**BOQ Fiber work**

 **From HBL to Data center**

|  |  |  |
| --- | --- | --- |
| **S.No** | **Description** | **Qty** |
| 01 | FOC 6 core fiber Single  Mode  | 1800ft |
| 02 | Fiber Splicing  | 12 |
| 03 | Other Accessories  | 01 |
| 04 | FOC Laying charges  Already laid PVC Its pulled and laid with Duct rodder from city campus data center to HBL Block Switch room (Ground Floor) | 1800ft |